跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# NET_SDK_IVE_VEHICE_HEAD_INFO

### 结构体定义

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    typedef struct
    {
        unsigned int begin_flag;
        unsigned int item_cnt;
        unsigned int plate_cnt;
        long long relativeTime;
        long long absoluteTime;
        unsigned int softwareVersion;
        unsigned int softwareBuildDate;
        unsigned char testFlag;
        unsigned char expandInfoFlag;
        unsigned char resver1[2];
        unsigned int resver[1];
        unsigned int end_flag;
    } NET_SDK_IVE_VEHICE_HEAD_INFO;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct NET_SDK_IVE_VEHICE_HEAD_INFO
    {
        public UInt32 begin_flag;
        public UInt32 item_cnt;
        public UInt32 plate_cnt;
        public Int64 relativeTime;
        public Int64 absoluteTime;
        public UInt32 softwareVersion;
        public UInt32 softwareBuildDate;
        public byte testFlag;
        public byte expandInfoFlag;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 2)]
        public byte[] resver1;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U4, SizeConst = 1)]
        public UInt32[] resver;
        public UInt32 end_flag;
    }

### 功能描述

车牌识别报警回调消息头。

### 成员说明

成员 | 类型 | 说明
--- | --- | ---
begin_flag | unsigned int | 开始标识，0x5a5a5a5a。
item_cnt | unsigned int | `NET_SDK_IVE_VEHICE_ITEM_INFO`的个数。
plate_cnt | unsigned int | 检测到车牌个数。
relativeTime | long long | 检测源数据相对时间,相对时间。
absoluteTime | long long | 检测源数据当前时间,绝对时间。
softwareVersion | unsigned int | 软件版本号, 0xABCDEFGH，AB：厂家；CD：主版本；EFGH：子版本 厂商 1:欧姆龙 版本:V5.00。
softwareBuildDate | unsigned int | 软件生成日期，0xYYYYMMDD。
testFlag | unsigned char | 上报类型标识，0：正常上报；1：测试上报。
expandInfoFlag | unsigned char | 有无无扩展信息结构标识， 0：无扩展信息结构；1：有扩展信息结构。
resver1 | unsigned char[2] | 预留字段。
resver | unsigned int[1] | 预留字段。
end_flag | unsigned int | 结束标识，0xa5a5a5a5。

错误码