跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# NET_SDK_EditSmartEventConfig

### 接口定义

C++C#

    1
    2
    3
    4
    5
    6
    BOOL NET_SDK_EditSmartEventConfig(
        LONG lUserID,
        DWORD dwCommand,
        LONG lChannel,
        LPVOID lpInBuffer,
        DWORD dwInBufferSize);

    1
    2
    3
    4
    5
    6
    public static extern Boolean NET_SDK_EditSmartEventConfig(
        Int32 lUserID,
        UInt32 dwCommand,
        Int32 lChannel,
        IntPtr lpInBuffer,
        UInt32 dwInBufferSize);

### 功能描述

编辑智能事件参数配置（目前仅支持NVR）。

### 参数说明

参数 | 类型 | 说明
--- | --- | ---
lUserIDin | LONG | 用户ID，`NET_SDK_Login`或`NET_SDK_LoginEx`的返回值。
dwCommandin | DWORD | 智能事件类型。
lChannelin | LONG | 通道编号，从0开始，IPC设备此参数无效。
lpInBufferin | LPVOID | 输入数据。
dwInBufferSizein | DWORD | 输入大小。

### 返回值

- 类型：BOOL

- 说明：成功返回TRUE,失败返回FALSE。

### 备注

根据dwCommand 的不同，对应的lpInBuffer数据结构如下：

dwCommand 宏定义 | dwCommand 对应值 | dwCommand 含义 | 数据结构(lpInBuffer)定义
--- | --- | --- | ---
NET_SDK_SMART_EVENT_TYPE_PASSLINE | 0x17 | 按越线统计目标 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_TRAFFIC | 0x18 | 按区域统计目标 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_PEA_TARGET | 0x19 | 周界防范，区域入侵侦测 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_VSD | 0x1a | 视频二级结构化 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_NVR_AOIENTRY | 0x1e | 进入区域 for NVR | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_NVR_AOILEAVE | 0x1f | 离开区域 for NVR | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_PVD | 0x20 | 违停检测 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_LOITER | 0x21 | 徘徊检测 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_TRIPWIRE | 0x26 | 周界防范，跨界侦测 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`
NET_SDK_SMART_EVENT_TYPE_HEATMAP | 0x27 | 热力图 | `NET_SDK_IVE_COMMON_CFG` + ruleCfgCount * `NET_SDK_IVE_DETECT_RULE_CFG`

错误码