跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# DD_LIVE_DISPLAY

### 结构体定义

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    typedef struct _dd_live_display_
    {
        unsigned int iSize;
        unsigned int showTime;
        unsigned int showNetwork;
        unsigned int showHDD;
        unsigned int showUSB;
        unsigned short alarmInNum;
        unsigned short alarmOutNum;
        unsigned int showAlarmIn;
        unsigned int showAlarmOut;
        unsigned int cameraNum;
        unsigned char showCameraName[DD_MAX_CAMERA_NUM];
        unsigned char showRecordStatus[DD_MAX_CAMERA_NUM];
    } DD_LIVE_DISPLAY;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct DD_LIVE_DISPLAY
    {
        public UInt32 iSize;
        public UInt32 showTime;
        public UInt32 showNetwork;
        public UInt32 showHDD;
        public UInt32 showUSB;
        public UInt16 alarmInNum;
        public UInt16 alarmOutNum;
        public UInt32 showAlarmIn;
        public UInt32 showAlarmOut;
        public UInt32 cameraNum;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 128)]
        public byte[] showCameraName;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 128)]
        public byte[] showRecordStatus;
    }

### 功能描述

预览显示结构体。

### 成员说明

成员 | 类型 | 说明
--- | --- | ---
iSize | unsigned int | 本结构体长度。
showTime | unsigned int | 是否显示系统时间。
showNetwork | unsigned int | 是否显示网络状态。
showHDD | unsigned int | 是否显示硬盘信息。
showUSB | unsigned int | 是否显示移动存储器信息。
alarmInNum | unsigned short | 报警输入数目（只读）。
alarmOutNum | unsigned short | 报警输出数目（只读）。
showAlarmIn | unsigned int | 是否显示报警输入信息。
showAlarmOut | unsigned int | 是否显示报警输出信息。
cameraNum | unsigned int | 有效通道数目（只读）。
showCameraName | unsigned char[DD_MAX_CAMERA_NUM] | 是否显示通道名称。
showRecordStatus | unsigned char[DD_MAX_CAMERA_NUM] | 是否显示录像状态。

错误码