跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# NET_SDK_IVE_EventData_T

### 结构体定义

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    typedef struct
    {
        unsigned int type;
        unsigned int status;
        unsigned int width;
        unsigned int height;
        unsigned int dataLen;
        unsigned int targetCnt;
        unsigned int targetDataLen[40];
        LONGLONG releativePts;
        unsigned char extendFlag;
        unsigned char reserve1[3];
        unsigned int globalEnterCarCounter;
        unsigned int globalEnterPersonCounter;
        unsigned int globalEnterBikeCounter;
        unsigned int globalLeaveCarCounter;
        unsigned int globalLeavePersonCounter;
        unsigned int globalLeaveBikeCounter;
        unsigned char reserve[36];
    } NET_SDK_IVE_EventData_T;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    23
    24
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct NET_SDK_IVE_EventData_T
    {
        public UInt32 type;
        public UInt32 status;
        public UInt32 width;
        public UInt32 height;
        public UInt32 dataLen;
        public UInt32 targetCnt;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U4, SizeConst = 40)]
        public UInt32[] targetDataLen;
        public Int64 releativePts;
        public byte extendFlag;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 3)]
        public byte[] reserve1;
        public UInt32 globalEnterCarCounter;
        public UInt32 globalEnterPersonCounter;
        public UInt32 globalEnterBikeCounter;
        public UInt32 globalLeaveCarCounter;
        public UInt32 globalLeavePersonCounter;
        public UInt32 globalLeaveBikeCounter;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 36)]
        public byte[] reserve;
    }

### 功能描述

事件数据原图结构体。

### 成员说明

成员 | 类型 | 说明
--- | --- | ---
type | unsigned int | 图片编码类型，0：JPG; 1：YUV。
status | unsigned int | 状态，0：invalid; 1：valid; 2：saved。
width | unsigned int | 图片宽度。
height | unsigned int | 图片高度。
dataLen | unsigned int | 图片数据长度。
targetCnt | unsigned int | 目标个数。
targetDataLen | unsigned int[40] | 每个目标的长度。
releativePts | LONGLONG | 相对时间戳。
extendFlag | unsigned char | 0 表示旧协议，不支持全局计数器，1表示支持全局计数器。
reserve1 | unsigned char[3] | 预留。
globalEnterCarCounter | unsigned int | 总进入车辆数，一直累计。
globalEnterPersonCounter | unsigned int | 总进入人数，一直累计。
globalEnterBikeCounter | unsigned int | 总进入非数，一直累计。
globalLeaveCarCounter | unsigned int | 总离开车辆数，一直累计。
globalLeavePersonCounter | unsigned int | 总离开车辆数，一直累计。
globalLeaveBikeCounter | unsigned int | 总离开车辆数，一直累计。
reserve | unsigned char[36] | 预留字段。

错误码