Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# DD_NETWORK_PLATFORM

### Structure Definition

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    typedef struct _network_platform
    {
        unsigned int CurrentPlat;
        unsigned int Switcher;
        unsigned int Port;
        unsigned int ReportId;
        char szAddress[16];
        unsigned int SwitchGB;
        unsigned int PortGB;
        unsigned int uLocalPort;
        char szRelm[16];
        char szAddressGB[16];
        char szUserName[16];
        char szPassword[16];
        char szDeviceIdGB[32];
        char szServerIdGB[32];
    } DD_NETWORK_PLATFORM;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    23
    24
    25
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct DD_NETWORK_PLATFORM
    {
        public UInt32 CurrentPlat;
        public UInt32 Switcher;
        public UInt32 Port;
        public UInt32 ReportId;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 16)]
        public byte[] szAddress;
        public UInt32 SwitchGB;
        public UInt32 PortGB;
        public UInt32 uLocalPort;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 16)]
        public byte[] szRelm;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 16)]
        public byte[] szAddressGB;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 16)]
        public byte[] szUserName;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 16)]
        public byte[] szPassword;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 32)]
        public byte[] szDeviceIdGB;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 32)]
        public byte[] szServerIdGB;
    }

### Function Description

Register the upper-level platform. N9000 supports both national standard and platform software. IPC can ignore the national standard.

### Member Description

Member | Type | Remark
--- | --- | ---
CurrentPlat | unsigned int | The current platform, the default is 1, indicating platform software, and 2 indicates national standard.
Switcher | unsigned int | Platform software, 1 means enabled, 0 means not enabled.
Port | unsigned int | Platform software, ports.
ReportId | unsigned int | Platform software, device ID.
szAddress | char[16] | Platform software, IP address.
SwitchGB | unsigned int | National standard, 1 means enabled, 0 means not enabled.
PortGB | unsigned int | National standard, port.
uLocalPort | unsigned int | National standard, local port.
szRelm | char[16] | National standard, sip server domain.
szAddressGB | char[16] | GB, address.
szUserName | char[16] | GB, user name.
szPassword | char[16] | National standard, password.
szDeviceIdGB | char[32] | National standard, device ID.
szServerIdGB | char[32] | National standard, sip server ID.

Error Code