Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# DD_ALARM_STATUS_INFO_Ex

### Structure Definition

C++C#

    1
    2
    3
    4
    5
    6
    7
    8
    typedef struct _alarm_status_ex
    {
        unsigned int iSize;
        int index;
        unsigned int alarmType;
        char alarmNode[32];
        char recv[32];
    } DD_ALARM_STATUS_INFO_Ex;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct DD_ALARM_STATUS_INFO_Ex
    {
        public UInt32 iSize;
        public Int32 index;
        public UInt32 alarmType;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 32)]
        public byte[] alarmNode;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 32)]
        public byte[] recv;
    }

### Function Description

Alarm status information extended structure.

### Member Description

Member | Type | Remark
--- | --- | ---
iSize | unsigned int | The length of this structure.
index | int | Alarm channel, alarms not related to the channel are -1, alarms related to the channel are channels, and alarms such as io are numbers.
alarmType | unsigned int | Alarm event type, NET_SDK_N9000_ALARM_TYPE_RAID_SUBHEALTH: array subhealthy NET_SDK_N9000_ALARM_TYPE_RAID_UNAVAILABLE: array unavailable.
alarmNode | char[32] | Alarm node.
recv | char[32] | Reserved Bytes

Error Code