跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# TEMPERATURE_ALARM_INFO_NEW

### 结构体定义

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    typedef struct
    {
        unsigned int dwRuleID;
        POINT_16 MaxTemperPos;
        int nMaxTemper;
        POINT_16 MinTemperPos;
        int nMinTemper;
        int nAverageTemper;
        unsigned int dwDegreeUnit;
        char szRuleName[64];
        unsigned int dwRuleType;
        unsigned int dwReserve[16];
        unsigned short usPolylinePointPos;
        unsigned short usPolylinePointNum;
        int chanel;
    } TEMPERATURE_ALARM_INFO_NEW;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct TEMPERATURE_ALARM_INFO_NEW
    {
        public UInt32 dwRuleID;
        public POINT_16 MaxTemperPos;
        public Int32 nMaxTemper;
        public POINT_16 MinTemperPos;
        public Int32 nMinTemper;
        public Int32 nAverageTemper;
        public UInt32 dwDegreeUnit;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 64)]
        public byte[] szRuleName;
        public UInt32 dwRuleType;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U4, SizeConst = 16)]
        public UInt32[] dwReserve;
        public UInt16 usPolylinePointPos;
        public UInt16 usPolylinePointNum;
        public Int32 chanel;
    }

### 功能描述

温度检测信息。

### 成员说明

成员 | 类型 | 说明
--- | --- | ---
dwRuleID | unsigned int | 规则ID。
MaxTemperPos | `POINT_16` | 温度最高点位置。
nMaxTemper | int | 温度最高点的温度。
MinTemperPos | `POINT_16` | 温度最低点位置。
nMinTemper | int | 温度最低点的温度。
nAverageTemper | int | 平均温度。
dwDegreeUnit | unsigned int | 温度单位，0：摄氏度；1：华氏度。
szRuleName | char[64] | 规则名。
dwRuleType | unsigned int | 规则类型，0：点；1：线；2：面。
dwReserve | unsigned int[16] | 预留字段。
usPolylinePointPos | unsigned short | 多段线描述点开始位置。
usPolylinePointNum | unsigned short | 多段线描述点数量。
chanel | int | 对应的通道号。

错误码