Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# NET_SDK_GetRecordStatus

### Interface Definition

C++C#

    1
    2
    3
    4
    LONG NET_SDK_GetRecordStatus(
        LONG lUserID,
        NET_SDK_RECORD_STATUS* pRecordStatus,
        LONG maxNum);

    1
    2
    3
    4
    public static extern Int32 NET_SDK_GetRecordStatus(
        Int32 lUserID,
        IntPtr pRecordStatus,
        Int32 maxNum);

### Function Description

Get the video status information (not supported by IPC).

### Parameter Description

Parameters | Type | Remark
--- | --- | ---
lUserIDin | LONG | User ID, the return value of `NET_SDK_Login` or `NET_SDK_LoginEx`.
pRecordStatusout | `NET_SDK_RECORD_STATUS`* | Recording status structure array.
maxNumin | LONG | The number of structures stored in pRecordStatus.

### Return Value

- Type：LONG

- Remark：The actual number of statuses returned.

### Remarks

None

Error Code