Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# NET_SDK_SMART_SUPPORT

### Structure Definition

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    23
    24
    25
    26
    27
    28
    struct NET_SDK_SMART_SUPPORT
    {
        BOOL supportAOIEntry;
        BOOL supportAOILeave;
        BOOL supportASD;
        BOOL supportAudioAlarmOut;
        BOOL supportAutoTrack;
        BOOL supportAvd;
        BOOL supportBinocularCount;
        BOOL supportCdd;
        BOOL supportCpc;
        BOOL supportFire;
        BOOL supportHeatMap;
        BOOL supportInvokeEventTypeConfig;
        BOOL supportIpd;
        BOOL supportLoitering;
        BOOL supportOsc;
        BOOL supportPassLine;
        BOOL supportPea;
        BOOL supportPvd;
        BOOL supportRegionStatistics;
        BOOL supportTemperature;
        BOOL supportTripwire;
        BOOL supportVehiclePlate;
        BOOL supportVfd;
        BOOL supportVideoMetadata;
        BOOL supportWhiteLightAlarmOut;
    };

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    18
    19
    20
    21
    22
    23
    24
    25
    26
    27
    28
    29
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct NET_SDK_SMART_SUPPORT
    {
        public bool supportAOIEntry;
        public bool supportAOILeave;
        public bool supportASD;
        public bool supportAudioAlarmOut;
        public bool supportAutoTrack;
        public bool supportAvd;
        public bool supportBinocularCount;
        public bool supportCdd;
        public bool supportCpc;
        public bool supportFire;
        public bool supportHeatMap;
        public bool supportInvokeEventTypeConfig;
        public bool supportIpd;
        public bool supportLoitering;
        public bool supportOsc;
        public bool supportPassLine;
        public bool supportPea;
        public bool supportPvd;
        public bool supportRegionStatistics;
        public bool supportTemperature;
        public bool supportTripwire;
        public bool supportVehiclePlate;
        public bool supportVfd;
        public bool supportVideoMetadata;
        public bool supportWhiteLightAlarmOut;
    }

### Function Description

Smart Event Support Information

### Member Description

Member | Type | Remark
--- | --- | ---
supportAOIEntry | BOOL | Whether to support regional entry
supportAOILeave | BOOL | Whether to support region leaving
supportASD | BOOL | Whether to support abnormal sound
supportAudioAlarmOut | BOOL | Whether to support audio alarm output
supportAutoTrack | BOOL | Whether to support automatic tracking
supportAvd | BOOL | Whether to support video anomaly detection
supportBinocularCount | BOOL | Whether to support binocular statistics
supportCdd | BOOL | Whether to support crowd density detection
supportCpc | BOOL | Whether to support traffic statistics
supportFire | BOOL | Whether to support fire point detection
supportHeatMap | BOOL | Whether to support heat map
supportInvokeEventTypeConfig | BOOL | Whether to support calling event type configuration
supportIpd | BOOL | Whether to support human intrusion detection
supportLoitering | BOOL | Whether to support wandering
supportOsc | BOOL | Whether to support item care
supportPassLine | BOOL | Whether to support over-the-line
supportPea | BOOL | Whether to support regional intrusion detection
supportPvd | BOOL | Whether to support illegal parking detection
supportRegionStatistics | BOOL | Whether to support regional statistics
supportTemperature | BOOL | Whether to support temperature detection
supportTripwire | BOOL | Whether to support tripwire detection
supportVehiclePlate | BOOL | Whether to support license plate detection
supportVfd | BOOL | Whether to support face detection
supportVideoMetadata | BOOL | Whether to support video secondary structuring
supportWhiteLightAlarmOut | BOOL | Whether to support white light alarm output

Error Code