Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# FIREPOINT_EVNET_INFO_T

### Structure Definition

C++C#

    1
    2
    3
    4
    5
    6
    7
    8
    typedef struct
    {
        unsigned int dwTargetID;
        unsigned char ucStatus;
        unsigned char ucReverse[3];
        RECT_16 Rect16;
        unsigned int dwReverse[32];
    } FIREPOINT_EVNET_INFO_T;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct FIREPOINT_EVNET_INFO_T
    {
        public UInt32 dwTargetID;
        public byte ucStatus;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U1, SizeConst = 3)]
        public byte[] ucReverse;
        public RECT_16 Rect16;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.U4, SizeConst = 32)]
        public UInt32[] dwReverse;
    }

### Function Description

Fire point information

### Member Description

Member | Type | Remark
--- | --- | ---
dwTargetID | unsigned int | Target ID.
ucStatus | unsigned char | Status, 0: none; 1: start; 2: end; 3: procedure.
ucReverse | unsigned char[3] | Reserved field.
Rect16 | `RECT_16` | The target rectangle.
dwReverse | unsigned int[32] | Reserved field.

Error Code