跳转至
本 SDK 仅适用于过去 3 年内发布的设备。我们定期优化和更新 SDK，以确保兼容性和性能。对于超过 3 年的旧设备，我们不保证兼容性，也不会提供技术支持。

# NET_SDK_IVE_PASSLINECOUNT_T

### 结构体定义

C++C#

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    typedef struct
    {
        unsigned int enterCarCount;
        unsigned int enterPersonCount;
        unsigned int enterBikeCount;
        unsigned int leaveCarCount;
        unsigned int leavePersonCount;
        unsigned int leaveBikeCount;
        unsigned int existCarCount;
        unsigned int existPersonCount;
        unsigned int existBikeCount;
        unsigned int count;
        NET_SDK_IVE_PASSLINECOUNT_INFO_T passLineInfo[32];
        GUID chlId;
    } NET_SDK_IVE_PASSLINECOUNT_T;

     1
     2
     3
     4
     5
     6
     7
     8
     9
    10
    11
    12
    13
    14
    15
    16
    17
    [StructLayout(LayoutKind.Sequential, Pack = 4)]
    public struct NET_SDK_IVE_PASSLINECOUNT_T
    {
        public UInt32 enterCarCount;
        public UInt32 enterPersonCount;
        public UInt32 enterBikeCount;
        public UInt32 leaveCarCount;
        public UInt32 leavePersonCount;
        public UInt32 leaveBikeCount;
        public UInt32 existCarCount;
        public UInt32 existPersonCount;
        public UInt32 existBikeCount;
        public UInt32 count;
        [MarshalAs(UnmanagedType.ByValArray, ArraySubType = UnmanagedType.Struct, SizeConst = 32)]
        public NET_SDK_IVE_PASSLINECOUNT_INFO_T[] passLineInfo;
        public GUID chlId;
    }

### 功能描述

过线统计消息。

### 成员说明

成员 | 类型 | 说明
--- | --- | ---
enterCarCount | unsigned int | 进入的车的辆数量。
enterPersonCount | unsigned int | 进入的人的数量。
enterBikeCount | unsigned int | 进入的自行车的数量。
leaveCarCount | unsigned int | 离开的车的辆数量。
leavePersonCount | unsigned int | 离开的人的数量。
leaveBikeCount | unsigned int | 离开的自行车的辆数量
existCarCount | unsigned int | 正在的车的数量。
existPersonCount | unsigned int | 正在的人的数量。
existBikeCount | unsigned int | 正在的自行车的数量。
count | unsigned int | 总数量，即passLineInfo的数量。
passLineInfo | `NET_SDK_IVE_PASSLINECOUNT_INFO_T`[32] | 过线分析结果列表。
chlId | GUID | 通道的GUID。

错误码