Skip to content
This SDK only works with devices released within the past 3 years. We regularly optimize and update the SDK to ensure compatibility and performance. We do not guarantee compatibility or provide technical support for devices older than 3 years.

# NET_SDK_StopDVRRecord

### Interface Definition

C++C#

    1
    2
    3
    BOOL NET_SDK_StopDVRRecord(
        LONG lUserID,
        LONG lChannel);

    1
    2
    3
    public static extern bool NET_SDK_StopDVRRecord(
        Int32 lUserID,
        int lChannel);

### Function Description

Remotely and manually stop device recording (supports N9000 only).

### Parameter Description

Parameters | Type | Remark
--- | --- | ---
lUserIDin | LONG | User ID, the return value of `NET_SDK_Login` or `NET_SDK_LoginEx`.
lChannelin | LONG | Channel number, starting from 0, 0x00ff means all analog channels, 0xff00 means all digital channels, and 0xffff means all analog and digital channels.

### Return Value

- Type：BOOL

- Remark：Returns TRUE if successful, FALSE if failed.

### Remarks

None

Error Code